

1. Power on STB, insert COM line to "RS-232" port of STB .
2. rename the upgrade file(GX6605\_SATCOM\_SC10MINI\_Release\_V3304.bin) to to "download\_ecos.bin", Copy "download\_ecos.bin" to U Disk, U Disk insert into STB.
3. Double click software named "GXDownloader\_boot\_V1.010.exe", it's parameters as shown in Figure



1. Click "START" button, wait 3 seconds, turn off STB, immediately turn on STB, STB is upgrading now.



1. When pop a dialog content "complete ", it means upgare finish, just restart STB, then use it as you want.

